Knauf 12.5mm Moisture Resistant Gypsum Board (MR) 1200 X 2400mm TE - H1

Knauf Hat Furring Channel (0.5mm gauge) / 3000mm length

Knauf Main Channel (0.5mm gauge) / 3000mm length

Knauf L Angle Section (0.5mm gauge) / 3000mm length - Plenum Depth of 1000mm

Knauf UD23/22 Channel (0.5mm gauge) / 3000mm length

Knauf LN4.2x11 Waferhead Screws (1000pcs/pack)

Knauf TN25 Drywall Screws (1000pcs/pack)

Knauf Readygips Jointing and Finishing Compound (28kg/pail)

Knauf Fiberglass Joint Tape 50mm (90m/roll)

Knauf 6/40 Hammer Fixings (200pcs/pack)

Knauf 6/40 Ceiling Wedge Anchor (200pcs/pack)

USG Boral Perforated Gypsum Ceiling Tiles - 600x600x12.5mm thick with front side Vinyl coated RAL 9016 and white tissue backing Tegular Edge Tiles.

**Knauf Suspension - T15 Grids.**

Knauf Main Runner 3600mm (T15) - Qty 195 Nos. Knauf Cross Tee 600mm (T15) - Qty 1102 Nos. Knauf Cross Tee 1200mm (T15) - Qty 1102 Nos. Knauf Wall Angle 3000mm (T15) - Qty 195 Nos. (Ceiling Anchors & Hanger wires by others)

**Material Description**

**USG Boral Gypsum Ceiling Tiles with KNUAF Grids.**

**Ref:- C2**

**Material Description**

**KNAUF Moisture Resistance (MR-H1) Gypsum Ceiling.**

**Ref:- C1, C3 & C7.**

USG Boral Aluminium **CLIP IN 600x600x0.7mm thick, Perforated** diagonal round hole 1.8mm dia, colour RAL 9016.

**Clip-In suspensions.**

Spring Tee 0.6mm thick, 3mtr long Primary Channel 0.6mm, 3mtr long Wire Connecting Clip

Primary Channel Hanging Bracket Hanger Rod 3.5mm x 2000mm Ajustable Butterfly Clips - 4mm Wall Angle 3.6mtr long.

Cement Board 1200 x 2400 x 12mm thick

Knauf Hat Furring Channel (0.5mm gauge) / 3000mm length

Knauf Main Channel (0.5mm gauge) / 3000mm length

Knauf L Angle Section (0.5mm gauge) / 3000mm length - Plenum Depth of 1000mm

Knauf UD23/22 Channel (0.5mm gauge) / 3000mm length

Knauf LN4.2x11 Waferhead Screws (1000pcs/pack)

Knauf Aquapanel Maxi Screw SN25 (1000pcs/pack)

Knauf 6/40 Hammer Fixings (200pcs/pack)

Knauf 6/40 Ceiling Wedge Anchor (200pcs/pack)

(Jointing Compound, Tapes, Skim Coating by others.)

**Material Description**

**Cement Board Ceiling.**

**Material Description**

**USG Boral Clip-In Aluminium Ceiling Tiles.**

Knauf 15mm Fire Resistant Gypsum Board (FR) 1200 X 2400mm TE

Knauf CW70/35 Stud (0.6mm gauge) / 3000mm length

Knauf UW70/32 Track (0.6mm gauge) / 3000mm length

Knauf UW70/60 Track (0.6mm gauge) / 3000mm length

Knauf LN4.2x11 Waferhead Screws (1000pcs/pack)

Knauf TN25 Drywall Screws (1000pcs/pack)

Knauf Readygips Jointing and Finishing Compound (28kg/pail)

Knauf Fiberglass Joint Tape 50mm (90m/roll)

Knauf 6/40 Hammer Fixings (200pcs/pack)

Knauf 6/40 Ceiling Wedge Anchor (200pcs/pack)

Knauf FR Sealant (280ml/tube)

Knauf 15mm Fire Resistant Gypsum Board (FR) 1200 X 2400mm TE

Knauf CW70/35 Stud (0.6mm gauge) / 3000mm length

Knauf UW70/32 Track (0.6mm gauge) / 3000mm length

Knauf UW70/60 Track (0.6mm gauge) / 3000mm length

Knauf LN4.2x11 Waferhead Screws (1000pcs/pack)

Knauf TN25 Drywall Screws (1000pcs/pack)

Knauf Readygips Jointing and Finishing Compound (28kg/pail)

Knauf Fiberglass Joint Tape 50mm (90m/roll)

Knauf 6/40 Hammer Fixings (200pcs/pack)

Knauf 6/40 Ceiling Wedge Anchor (200pcs/pack)

Knauf FR Sealant (280ml/tube)

**Material Description**

**KNAUF KW-B111- 100mm Drywall Partitions Single Stud and Single Layer Boarding System.**

**Material Description**

**KNAUF KW-B116 - 200mm Drywall Partitions**

**Double Stud and Single Layer Board system Reinforced with Strips.**